Before proceeding with an erase flash procedure, please be sure to document all settings such as swath width and custom NMEA settings as you will be returning the console to its factory default settings. You may re-enter your settings at the end of this procedure.

1. Disconnect the antenna input from the side of console.
2. Press “***Stop Guidance***” and then “***Enter***” quickly one after another- This may take several attempts.
3. A menu will appear: “***BD Menu – Keyboard Test***”.
4. Use the down arrow until the cursor points to “***Erase Flash***”.
5. Press “**Enter**”- The console will display “***Erasing Flash***” and it will count down from 20 and the LED’s will cycle through once.
6. Turn off the unit, re-attach the antenna, and power the unit back on
7. Press “***Menu***”, scroll down to “***Service Menu***”, then press “**Enter**”.
8. Scroll down to “***Reset Defaults****”,* and then press “**Enter**” again.
9. The Menu will display “***Reset Defaults – Press Enter to Reset***”-
10. Press “***Enter***” and the console will now go back to the default settings.
11. Now Press the “***Menu***” button two times and it will return you to home screen.
12. You may now re-enter your swath width and any custom settings you may have had.